initialisation

Read input data from joystick

Compare with reference value

no

Send data to motor driver

Movement of motor in forward direction

Check Vrx,Vry

Movement of motor in reverse direction